LOGNAME=  data.log
ACTION= 1
PROMPT= 1
NCORES=  8

INSET=  eso121-g6.fts
BOX= 

# change output name
OUTSET= eso121-g6_out_01.fts
OUTCUBUP= 10000000.0

PROGRESSLOG= 
TEXTLOG= 

BMIN= 
BMAJ= 
BPA= 
RMS=  0.002

NDISKS=  2
NUR= 11
    RADI= +0.00000E+00 +2.00000E+01 +4.00000E+01 +6.00000E+01 +8.00000E+01 +1.00000E+02 +1.20000E+02 +1.40000E+02 +1.60000E+02 +1.80000E+02 +2.00000E+02 
    VROT= +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 
      Z0= +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 
     SBR= +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 
    AZ1W= +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 
    INCL= +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 
      PA= +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 
    XPOS= +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 
    YPOS= -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 
    VSYS= +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 
  VROT_2= +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 +1.41598E+02 
    Z0_2= +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 +9.40054E+00 
   SBR_2= +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 +2.95172E-04 
  AZ1P_2= +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 
  AZ1W_2= +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 +1.80000E+02 
  INCL_2= +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 +8.58497E+01 
    PA_2= +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 +3.81847E+01 
  XPOS_2= +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 +9.18746434E+01 
  YPOS_2= -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 -6.18077071E+01 
  VSYS_2= +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 +1.18932E+03 
 CONDISP= +1.92962E+01 
LTYPE=  2.0
LTYPE_2= 

CFLUX=  2e-06
CFLUX_2= 
PENALTY=  1.0
WEIGHT=  0
RADSEP=  0.05
INIMODE= 
ISEED=  8981

FITMODE=  2
LOOPS=  4
MAXITER= 
CALLITE= 
SIZE=  4

# now we start to fit for single rings, but we leave out every second ring for position angle, rotation velocity, and inclination, for position angle and inclination, rings 1-4 adopt the values of ring 5 (flat inner disk), surface brightness is fitted at full resolution (and is hence left out in the VARINDX list)
VARINDX=   PA 1 3 2:10:2 PA_2 1 3 2:10:2 VROT 2:10:2 VROT_2 2:10:2 INCL 1 3 2:10:2 INCL_2 1 3 2:10:2 
# fit now at independent radii surface brightness, rotation velocity, position angle, and inclination
VARY=       ! SBR 1:11 SBR_2 1:11, ! VROT 1:11 VROT_2 1:11, ! PA 1:11 PA_2 1:11, ! INCL  1:11 INCL_2  1:11, Z0  1:11 Z0_2  1:11,  XPOS 1:11 XPOS_2 1:11, YPOS 1:11 YPOS_2 1:11, VSYS  1:11  VSYS_2  1:11, CONDISP
PARMAX=                         1                      800                  360                        180                  100                     360                    180                     10000       80
PARMIN=                         0                        0                    0                          0                    0                       0                   -180                         1        1
MODERATE=                       3                        3                    3                          3                    3                       3                      3                         3        3
DELSTART=                    5E-6                        3                    2                          2                    5                   0.005                  0.005                       0.5        2
DELEND=                      5E-6                        2                    1                          1                    1                   0.001                  0.001                       0.2        1
ITESTART=                      70                       70                   70                         70                   70                      70                     70                        70       70
ITEEND=                        70                       70                   70                         70                   70                      70                     70                        70       70
SATDELT=                     1E-6                      0.2                  0.2                        0.2                    2                  0.0005                 0.0005                      0.05     0.05
MINDELTA=                    5E-7                     0.05                 0.05                       0.05                    1                  0.0002                 0.0002                      0.02     0.02
REGPARA= 

# change output name
TIRDEF= eso121-g6_out_01.def
TIRSMO= 

COOLGAL= 
COOLBEAM=  20

TILT= 
BIGTILT= 


# change output name
GR_DEVICE= eso121-g6_01.ps/vcps
GR_PARMS=  RADI SBR VROT PA INCL
GR_XMIN= 
GR_XMAX= 
GR_MR=  5
GR_ML=  5
GR_TXHT=  1
GR_SBHT=  0.5
GR_LGND=  1
GR_SBRP=  0

GR_COL_1=  1
GR_LINES_1=  1
GR_ERRB_1= 
GR_YMIN_1= 
GR_YMAX_1= 

GR_COL_2=  1
GR_LINES_2=  1
GR_ERRB_2= 
GR_YMIN_2= 
GR_YMAX_2= 

GR_COL_3=  1
GR_LINES_3=  1
GR_ERRB_3= 
GR_YMIN_3= 
GR_YMAX_3= 

GR_COL_4=  1
GR_LINES_4=  1
GR_ERRB_4= 
GR_YMIN_4= 
GR_YMAX_4= 
